
1. CCNA Security

Lab – 4.4.1.2 Configuring Zone-Based Policy Firewalls

1. Topology



1. IP Addressing Table

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| Device | Interface | IP Address | Subnet Mask | Default Gateway | Switch Port |
| R1 | G0/0/1 | 192.168.1.1 | 255.255.255.0 | N/A | S3 G1/0/11 |
|  | S0/1/0 (DCE) | 10.1.1.1 | 255.255.255.252 | N/A | N/A |
| R2 | S0/1/0 | 10.1.1.2 | 255.255.255.252 | N/A | N/A |
|  | S0/1/1 (DCE) | 10.2.2.2 | 255.255.255.252 | N/A | N/A |
| R3 | G0/0/0 | 192.168.33.1 | 255.255.255.0 | N/A | N/A |
|  | G0/0/1 | 192.168.3.1 | 255.255.255.0 | N/A | S4 G1/0/11 |
|  | S0/0/1 | 10.2.2.1 | 255.255.255.252 | N/A | N/A |
| PC-A | NIC | 192.168.1.3 | 255.255.255.0 | 192.168.1.1 | S3 G1/0/13 |
| PC-B | NIC | 192.168.3.3 | 255.255.255.0 | 192.168.3.1 | S4 F0/24 |
| PC-C | NIC | 192.168.33.3 | 255.255.255.0 | 192.168.33.1 | N/A |

1. Objectives

Part 1: Basic Router Configuration

* Configure host names, interface IP addresses, and access passwords.
* Configure the static routes to enable end-to-end connectivity.

Part 2: Configuring a Zone-Based Policy Firewall (ZPF)

* Use the CLI to configure a Zone-Based Policy Firewall.
* Use the CLI to verify the configuration.

1. Background

The most basic form of a Cisco IOS firewall uses access control lists (ACLs) to filter IP traffic and monitor established traffic patterns. A traditional Cisco IOS firewall is an ACL-based firewall.

The newer Cisco IOS Firewall implementation uses a zone-based approach that operates as a function of interfaces instead of access control lists. A Zone-Based Policy Firewall (ZPF) allows different inspection policies to be applied to multiple host groups connected to the same router interface. It can be configured for extremely advanced, protocol specific, granular control. It prohibits traffic via a default deny-all policy between different firewall zones. ZPF is suited for multiple interfaces that have similar or varying security requirements.

In this lab, you build a multi-router network, configure the routers and PC hosts, and configure a Zone-Based Policy Firewall using the Cisco IOS command line interface (CLI).

**Note**: The router commands and output in this lab are from a Cisco 1941 with Cisco IOS Release 15.4(3)M2 (UniversalK9-M). Other routers and Cisco IOS versions can be used. See the Router Interface Summary Table at the end of the lab to determine which interface identifiers to use based on the equipment in the lab. Depending on the router model and Cisco IOS version, the commands available and output produced might vary from what is shown in this lab.

**Note**: Make sure that the routers and switches have been erased and have no startup configurations.

1. Required Resources

* 3 Routers (Cisco 1941 with Cisco IOS Release 15.4(3)M2 image or comparable)
* 2 Switches (Cisco 2960 or comparable)
* 3 PCs (Windows Vista or Windows 7)
* Serial and Ethernet cables, as shown in the topology
* Console cables to configure Cisco networking devices

1. Basic Router Configuration

In Part 1 of this lab, you set up the network topology and configure basic settings, such as the interface IP addresses, static routing, device access, and passwords.

**Note**: All tasks should be performed on routers R1, R2, and R3. The procedures are shown for only one of the routers.

* + 1. Cable the network as shown in the topology.

Attach the devices as shown in the topology diagram, and cable as necessary.

* + 1. Configure basic settings for each router.

a. Configure host names as shown in the topology.

b. Configure the interface IP addresses as shown in the IP addressing table.

c. Configure a clock rate for the serial router interfaces with a DCE serial cable attached.

R2(config)# **interface S0/1/0**

R2(config-if)# **clock rate 64000**

* + 1. Disable DNS lookup.

To prevent the router from attempting to translate incorrectly entered commands, disable DNS lookup.

R2(config)# **no ip domain-lookup**

* + 1. Configure static routes on R1, R2, and R3.
       1. In order to achieve end-to-end IP reachability, proper static routes must be configured on R1, R2 and R3. R1 and R3 are stub routers, and as such, only need a default route pointing to R2. R2, behaving as the ISP, must know how to reach R1’s and R3’s internal networks before end-to-end IP reachability is achieved. Below is the static route configuration for R1, R2 and R3. On R1, use the following command:

R1(config)# **ip route 0.0.0.0 0.0.0.0 10.1.1.2**

* + - 1. On R2, use the following commands.

R2(config)# **ip route 192.168.1.0 255.255.255.0 10.1.1.1**

R2(config)# **ip route 192.168.3.0 255.255.255.0 10.2.2.1**

R2(config)# **ip route 192.168.33.0 255.255.255.0 10.2.2.1**

* + - 1. On R3, use the following command.

R3(config)# **ip route 0.0.0.0 0.0.0.0 10.2.2.2**

* + 1. Configure PC host IP settings.

Configure a static IP address, subnet mask, and default gateway for PC-A, PC-B, and PC-C as shown in the IP addressing table.

* + 1. Verify basic network connectivity.
       1. Ping from R1 to R3.

If the pings are not successful, troubleshoot the basic device configurations before continuing.

* + - 1. Ping from PC-A on the R1 LAN to PC-C on the R3 LAN.

If the pings are not successful, troubleshoot the basic device configurations before continuing.

**Note**: If you can ping from PC-A to PC-C, you have demonstrated that the end-to-end IP reachability has been achieved. If you cannot ping but the device interfaces are UP and IP addresses are correct, use the **show interface**, **show ip interface,** and **show ip route** commands to help identify problems.

* + 1. Configure a user account, encrypted passwords and crypto keys for SSH.

**Note**: Passwords in this task are set to a minimum of 10 characters, but are relatively simple for the benefit of performing the lab. More complex passwords are recommended in a production network.

* + - 1. Configure a minimum password length using the **security passwords** command to set a minimum password length of 10 characters.

R1(config)# **security passwords min-length 10**

* + - 1. Configure a domain name.

R1(config)# **ip domain-name ccnasecurity.com**

* + - 1. Configure crypto keys for SSH

R1(config)# **crypto key generate rsa general-keys modulus 1024**

* + - 1. Configure an admin01 user account using **algorithm-type scrypt** for encryption and a password of cisco12345.

R1(config)# **username admin01 algorithm-type scrypt secret cisco12345**

* + - 1. Configure line console 0 to use the local user database for logins. For additional security, the **exec-timeout** command causes the line to log out after **5** minutes of inactivity. The **logging synchronous** command prevents console messages from interrupting command entry.

**Note**: To avoid repetitive logins during this lab, the **exec-timeout** command can be set to **0 0**, which prevents it from expiring; however, this is not considered to be a good security practice.

R1(config)# **line console 0**

R1(config-line)# **login local**

R1(config-line)# **exec-timeout 5 0**

R1(config-line)# **logging synchronous**

* + - 1. Configure line aux 0 to use the local user database for logins.

R1(config)# **line aux 0**

R1(config-line)# **login local**

R1(config-line)# **exec-timeout 5 0**

* + - 1. Configure line vty 0 4 to use the local user database for logins and restrict access to SSH connections only.

R1(config)# **line vty 0 4**

R1(config-line)# **login local**

R1(config-line)# **transport input ssh**

R1(config-line)# **exec-timeout 5 0**

* + - 1. Configure the enable password with strong encryption.

R1(config)# **enable algorithm-type scrypt secret class12345**

* + 1. Save the basic running configuration for all three routers.

Save the running configuration to the startup configuration from the privileged EXEC prompt.

R1# **copy running-config startup-config**

1. Configuring a Zone-Based Policy Firewall (ZPF)

The ISR G2 4321 may not have had the securityk9 package activated.

To check:

R3# show license feature

Look for

Feature name Enforcement Evaluation Subscription Enabled RightToUse

Securityk9 yes yes no no yes

If it is not enabled perform the following:

To activate

R3(config)# license boot level securityk9

R3(config)# exit

R3# write

R3# reload

In Part 2 of this lab, you configure a zone-based policy firewall (ZPF) on R3 using the command line interface (CLI).

* 1. Verify Current Router Configurations.

In this task, you will verify end-to-end network connectivity before implementing ZPF.

* + 1. Verify end-to-end network connectivity.
       1. Ping from R1 to R3 Using both of R3’s Gigabit Ethernet interface IP addresses.

If the pings are not successful, troubleshoot the basic device configurations before continuing.

* + - 1. Ping from PC-A on the R1 LAN to PC-C on the R3 conference room LAN.

If the pings are not successful, troubleshoot the basic device configurations before continuing.

* + - 1. Ping from PC-A on the R1 LAN to PC-B on the R3 internal LAN.

If the pings are not successful, troubleshoot the basic device configurations before continuing.

* + 1. Display the R3 running configurations.
       1. Issue the **show ip interface brief** command on R3 to verify the correct IP addresses were assigned. Use the IP Address Table to verify the addresses.
       2. Issue the **show ip route** command on R3 to verify it has a static default route pointing to R2’s serial 0/1/1 interface.
       3. Issue the **show run** command to review the current basic configuration on R3.
       4. Verify the R3 basic configuration as performed in Part 1 of the lab. Are there any security commands related to access control?

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* 1. Create a Zone-Based Policy Firewall

In this task, you will create a zone-based policy firewall on R3, making it act not only as a router but also as a firewall. R3 is currently responsible for routing packets for the three networks connected to it. R3’s interface roles are configured as follows:

Serial 0/0/1 is connected to the Internet. Because this is a public network, it is considered an *untrusted* network and should have the lowest security level.

G0/1 is connected to the internal network. Only authorized users have access to this network. In addition, vital institution resources also reside in this network. The internal network is to be considered a *trusted* network and should have the highest security level.

G0/0 is connected to a conference room. The conference room is used to host meetings with people who are not part of the organization.

The security policy to be enforced by R3 when it is acting as a firewall dictates that:

* No traffic initiated from the Internet should be allowed into the internal or conference room networks.
* Returning Internet traffic (return packets coming from the Internet into the R3 site, in response to requests originating from any of the R3 networks) should be allowed.
* Computers in the R3 internal network are considered *trusted* and are allowed to initiate any type traffic (TCP, UDP or ICMP based traffic).
* Computers in the R3 conference room network are considered *untrusted* and are allowed to initiate only web traffic (HTTP or HTTPS) to the Internet.
* No traffic is allowed between the internal network and the conference room network. There is no guarantee regarding the condition of guest computers in the conference room network. Such machines could be infected with malware and might attempt to send out spam or other malicious traffic.
  + 1. Creating the security zones.

A security zone is a group of interfaces with similar security properties and requirements. For example, if a router has three interfaces connected to internal networks, all three interfaces can be placed under the same zone named “internal”. Because all security properties are configured to the zone instead of to the individual router interfaces, the firewall design is much more scalable.

In this lab, the R3 site has three interfaces; one connected to an internal trusted network, one connected to the conference room network and another connected to the Internet. Because all three networks have different security requirements and properties, we will create three different security zones.

* + - 1. Security zones are created in global configuration mode, and the command allows for zone name definition. In R3, create three zones named **INSIDE**, **CONFROOM** and **INTERNET**:

R3(config)# **zone security INSIDE**

R3(config)# **zone security CONFROOM**

R3(config)# **zone security INTERNET**

* + 1. Creating Security Policies

Before ZPF can decide if some specific traffic should be allowed or denied, it must be told *what* traffic is to be considered. Cisco IOS uses class-maps to select traffic. *Interesting traffic* is a common denomination for traffic that has been selected by a class-map.

While class-maps select traffic, it is not their job to decide what happens to the selected traffic; Policy-maps decide the *fate* of the selected traffic.

ZPF traffic policies are defined as policy-maps and use class-maps to select traffic. In other words, class-maps define *what* traffic is to be policed while policy-maps define the *action* to be taken upon the selected traffic.

Policy-maps can drop, pass or inspect traffic. Because we want the firewall to *watch* traffic moving in the direction of zone-pairs, we will create inspect policy-maps. Inspect policy-maps allow for dynamic handling of the return traffic.

First, you will create class-maps. After the class-maps are created, you will create policy-maps and attach the class-maps to the policy-maps.

* + - 1. Create an inspect class-map to match traffic to be allowed from the INSIDE zone to the **INTERNET** zone. Because we trust the INSIDE zone, we allow all the main protocols.

In the commands below, the first line creates an inspect class-map. The **match-any** keyword instructs the router that any of the **match** protocol statements will qualify as a successful match resulting in a policy being applied. The result is a match for TCP or UDP or ICMP packets.

The **match** commands refer to specific Cisco NBAR supported protocols. For more information on Cisco NBAR visit [Cisco Network-Based Application Recognition](http://www.cisco.com/c/en/us/products/collateral/ios-nx-os-software/network-based-application-recognition-nbar/prod_case_study09186a00800ad0ca.html).

R3(config)# **class-map type inspect match-any INSIDE\_PROTOCOLS**

R3(config-cmap)# **match protocol tcp**

R3(config-cmap)# **match protocol udp**

R3(config-cmap)# **match protocol icmp**

* + - 1. Similarly, create a class-map to match the traffic to be allowed from the **CONFROOM** zone to the **INTERNET** zone. Because we do not fully trust the **CONFROOM** zone, we must limit what the server can send out to the Internet:

R3(config)# **class-map type inspect match-any CONFROOM\_PROTOCOLS**

R3(config-cmap)# **match protocol http**

R3(config-cmap)# **match protocol https**

R3(config-cmap)# **match protocol dns**

* + - 1. Now that the class-maps are created, you can create the policy-maps.

In the commands below, the first line creates an inspect policy-map named **INSIDE\_TO\_INTERNET**. The second line binds the previously created **INSIDE\_PROTOCOLS** class-map to the policy-map. All packets matched by the **INSIDE\_PROTOCOLS** class-map will be subjected to the action taken by the **INSIDE\_TO\_INTERNET** policy-map. Finally, the third line defines the actual action this policy-map will apply to the matched packets. In this case, the matched packets will be inspected.

The next three lines creates a similar policy-map named **CONFROOM\_TO\_INTERNET** and attaches the **CONFROOM\_PROTOCOLS** class-map.

The commands are as follows:

R3(config)# **policy-map type inspect INSIDE\_TO\_INTERNET**

R3(config-pmap)# **class type inspect INSIDE\_PROTOCOLS**

R3(config-pmap-c)# **inspect**

R3(config)# **policy-map type inspect CONFROOM\_TO\_INTERNET**

R3(config-pmap)# **class type inspect CONFROOM\_PROTOCOLS**

R3(config-pmap-c)# **inspect**

* + 1. Create the Zone Pairs

A zone pair allows you to specify a unidirectional firewall policy between two security zones.

For example, a commonly used security policy dictates that the internal network can initiate any traffic towards the Internet but no traffic originating from the Internet should be allowed to reach the internal network.

This traffic policy requires only one zone pair, **INTERNAL to INTERNET**. Because zone-pairs define unidirectional traffic flow, another zone-pair must be created if Internet-initiated traffic must flow in the **INTERNET to INTERNAL** direction.

Notice that Cisco ZPF can be configured to inspect traffic that moves in the direction defined by the zone pair. In that situation, the firewall *watches* the traffic and dynamically creates rules allowing the return or related traffic to flow back through the router.

To define a zone pair, use the **zone-pair security** command. The direction of the traffic is specified by the source and destination zones.

For this lab, you will create two zone-pairs:

**INSIDE\_TO\_INTERNET:** Allows traffic leaving the internal network towards the Internet.

**CONFROOM\_TO\_INTERNET:** Allows Internet access from the ConfRoom network.

* + - 1. Creating the zone-pairs:

R3(config)# **zone-pair security INSIDE\_TO\_INTERNET source INSIDE destination INTERNET**

R3(config)# **zone-pair security CONFROOM\_TO\_INTERNET source CONFROOM destination INTERNET**

* + - 1. Verify the zone-pairs were correctly created by issuing the **show zone-pair security** command. Notice that no policies are associated with the zone-pairs yet. The security policies will be applied to zone-pairs in the next step.

R3# **show zone-pair security**

Zone-pair name INSIDE\_TO\_INTERNET

Source-Zone INSIDE Destination-Zone INTERNET

service-policy not configured

Zone-pair name CONFROOM\_TO\_INTERNET

Source-Zone CONFROOM Destination-Zone INTERNET

service-policy not configured

* + 1. Applying Security Policies
       1. As the last configuration step, apply the policy-maps to the zone-pairs:

R3(config)# **zone-pair security INSIDE\_TO\_INTERNET**

R3(config-sec-zone-pair)# **service-policy type inspect INSIDE\_TO\_INTERNET**

R3(config)# **zone-pair security CONFROOM\_TO\_INTERNET**

R3(config-sec-zone-pair)# **service-policy type inspect CONFROOM\_TO\_INTERNET**

* + - 1. Issue the **show** **zone-pair security** command once again to verify the zone-pair configuration. Notice that the service-polices are now displayed:

R3#**show zone-pair security**

Zone-pair name INSIDE\_TO\_INTERNET

Source-Zone INSIDE Destination-Zone INTERNET

service-policy INSIDE\_TO\_INTERNET

Zone-pair name CONFROOM\_TO\_INTERNET

Source-Zone CONFROOM Destination-Zone INTERNET

service-policy CONFROOM\_TO\_INTERNET

To obtain more information about the zone-pairs, their policy-maps, the class-maps and match counters, use the **show policy-map type inspect zone-pair** command:

R3#**show policy-map type inspect zone-pair**

policy exists on zp INSIDE\_TO\_INTERNET

Zone-pair: INSIDE\_TO\_INTERNET

Service-policy inspect : INSIDE\_TO\_INTERNET

Class-map: INSIDE\_PROTOCOLS (match-any)

Match: protocol tcp

0 packets, 0 bytes

30 second rate 0 bps

Match: protocol udp

0 packets, 0 bytes

30 second rate 0 bps

Match: protocol icmp

0 packets, 0 bytes

30 second rate 0 bps

Inspect

Session creations since subsystem startup or last reset 0

Current session counts (estab/half-open/terminating) [0:0:0]

Maxever session counts (estab/half-open/terminating) [0:0:0]

Last session created never

Last statistic reset never

Last session creation rate 0

Maxever session creation rate 0

Last half-open session total 0

TCP reassembly statistics

received 0 packets out-of-order; dropped 0

peak memory usage 0 KB; current usage: 0 KB

peak queue length 0

Class-map: class-default (match-any)

Match: any

Drop

0 packets, 0 bytes

[output omitted]

* + 1. Assign Interfaces to the Proper Security Zones

Interfaces (physical and logical) are assigned to security zones with the **zone-member security** interface command.

* + - 1. Assign R3’s G0/0/0 to the **CONFROOM** security zone:

R3(config)# **interface g0/0/0**

R3(config-if)# **zone-member security CONFROOM**

* + - 1. Assign R3’s G0/0/1 to the INSIDE security zone:

R3(config)# **interface g0/0/1**

R3(config-if)# **zone-member security INSIDE**

* + - 1. Assign R3’s S0/1/1 to the **INTERNET** security zone:

R3(config)# **interface s0/1/1**

R3(config-if)# **zone-member security INTERNET**

* + 1. Verify Zone Assignment
       1. Issue the show zone security command to ensure the zones were properly created, and the interfaces were correctly assigned:

R3# **show zone security**

zone self

Description: System defined zone

zone CONFROOM

Member Interfaces:

GigEthernet0/0/0

zone INSIDE

Member Interfaces:

GigEthernet0/0/1

zone INTERNET

Member Interfaces:

Serial0/1/1

* + - 1. Even though no commands were issued to create a “self” zone, the output above still displays it. Why is R3 displaying a zone named “self”? What is the significance of this zone?

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. ZPF Verification
   1. Verify ZPF Firewall Functionality
      1. Traffic originating on the Internet
2. To test the firewall’s effectiveness, ping PC-B from PC-A. In PC-A, open a command prompt and issue:

**C:\Users\NetAcad> ping 192.168.3.3**

Was the ping successful? Explain.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Ping PC-C from PC-A. In PC-A, open a command window and issue

**C:\Users\NetAcad> ping 192.168.33.3**

Was the ping successful? Explain.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Ping PC-A from PC-B. In PC-B, open a command window and issue

**C:\Users\NetAcad> ping 192.168.1.3**

1. Was the ping successful? Explain.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Ping PC-A from PC-C. In PC-C, open a command window and issue

**C:\Users\NetAcad> ping 192.168.1.3**

1. Was the ping successful? Explain.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

* + 1. The Self Zone Verification

1. From PC-A ping R3’s G0/0/1 interface:

C**:\Users\NetAcad**> **ping 192.168.3.1**

Was the ping successful? Is this the correct behavior? Explain.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. From PC-C ping R3’s G0/0/1 interface:

C**:\Users\NetAcad**> **ping 192.168.3.1**

Was the ping successful? Is this the correct behavior? Explain.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

1. Challenge (optional)

Create the proper zone-pair, class-maps, and policy-maps and configure R3 to prevent Internet originating traffic from reaching the Self Zone.

1. Appendix – Multiple Interfaces under the Same Zone (optional)

One benefit of ZPF firewalls is that they scale well compared to the classic firewall. If a new interface with the same security requirements is added to the firewall, the administrator can simply add the new interface as a member of an existing security zone. However, some IOS versions will not allow devices connected to different interfaces of the same zone to communicate by default. In those cases, a zone-pair must be created using the same zone as source and destination.

Traffic between similarly zoned interfaces will always be bidirectional due the fact that the zone-pair’s source and destination zones are the same. Because of that, there is no need to inspect traffic to allow for automatic return traffic handling; return traffic will always be allowed because it will always conform to the zone-pair definition. In this case, the policy-map should have a **pass** action instead of **inspect**. Because of the **pass** action, the router will not inspect packets matched by the policy-map, it will simply forward it to its destination.

In the context of this lab, if R3 had a G0/0/2 interface also assigned to the INSIDE zone, and the router IOS version did not suppport allowing traffic between interfaces configured to the same zone, the extra configuration would look like this:

New zone-pair: **Inside to Inside**; allows routing of traffic among the internal trusted interfaces.

Creating the policy-map (notice that no explicit class-map is needed because we use the default “catch-all” class):

R3(config)# **policy-map type inspect inside**

R3(config-pmap)# **class class-default**

R3(config-pmap-c)# **pass**

Creating the zone-pair and assigning the new policy-map to it. Notice that the INSIDE zone is both the source and the destination of the zone-pair:

R3(config)# **zone-pair security INSIDE source INSIDE destination INSIDE**

R3(config-sec-zone-pair)# **service-policy type inspect inside**

To verify the existence of the new pair, use **show zone-pair security:**

R3# **show zone-pair security**

Zone-pair name INSIDE\_TO\_INTERNET

Source-Zone INSIDE Destination-Zone INTERNET

service-policy INSIDE\_TO\_INTERNET

Zone-pair name CONFROOM\_TO\_INTERNET

Source-Zone CONFROOM Destination-Zone INTERNET

service-policy CONFROOM\_TO\_INTERNET

Zone-pair name INSIDE

Source-Zone INSIDE Destination-Zone INSIDE

service-policy inside

1. Router Interface Summary Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Router Interface Summary | | | | |
| Router Model | Ethernet Interface #1 | Ethernet Interface #2 | Serial Interface #1 | Serial Interface #2 |
| 1800 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 1900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2801 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 2811 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| **Note**: To find out how the router is configured, look at the interfaces to identify the type of router and how many interfaces the router has. There is no way to effectively list all the combinations of configurations for each router class. This table includes identifiers for the possible combinations of Ethernet and Serial interfaces in the device. The table does not include any other type of interface, even though a specific router may contain one. An example of this might be an ISDN BRI interface. The string in parenthesis is the legal abbreviation that can be used in Cisco IOS commands to represent the interface. | | | | |